Neu in MIKE URBAN Version 2017

Mit MIKE URBAN 2017 wird ArcGIS Version 10.5 installiert. Falls Sie in Ihrem Unternehmen unabhängig davon ArcGIS 10.5.1 installieren, ist auch dies in Kombination mit MIKE URBAN 2017 möglich.

- MIKE 1D Oberflächenabfluss Modell B (Kinematische Welle) wurde überprüft und einer kompletten Überarbeitung unterzogen, insbesondere in Bezug auf Verdunstung, Infiltration und die Horton-Ansätze. Die folgenden Änderungen sind enthalten:

Reihenfolge der Drainage hat sich geändert

Die Begrenzung der Versickerung durch Regen wurde deaktiviert

Die Wiedergewinnung des Versickerungspotentials wurde aktualisiert

Eine weitere Optimierung der LTS-Simulationen mit MIKE 1D wurde durchgeführt, um kleinere Ergebnisdateien zu erzeugen und den Systemspeicher optimal zu nutzen.

MIKE URBAN 2017, Service Pack 2 (SP2), April 2018

Modul/Typ	Neues Feature/Fehler	Status
MIKE 1D	Fließgeschwindigkeiten sind nun in der res1d-Ergebnisdatei standardmäßig enthalten	Fixed
MIKE 1D	MIKE 1D Die Geschwindigkeit bei der Berechnung des Oberflächenabflusses wurde erhöht und Ergebnisdatei verkleinert für LTS .	Fixed
MIKE 1D	Die Erkennung des Startkriteriums MIKE 1D LTS Joblistengenerierung wurde an das in Österreich verwendete Regen-Datenformat angepasst (lokaler Wetterdienst, ZAMG).	Fixed
MIKE 1D	LTS-Simulation mit monatlicher Abfluss- und Emissionsstatistik führte zum Absturz von MIKE URBAN	Fixed
MIKE 1D	Veraltete Abschnitte in der LTS-Statistik-Ergebnisdatei, erf	Fixed
MIKE 1D	MIKE 1D LTS ist relativ langsam bei der Erstellung von Job-Listen, insbesondere in Modellen mit vielen Einzugsgebieten.	Fixed
MIKE 1D	Unterstützung von Sickerschächten in LTS	Fixed
MIKE 1D	MIKE 1D LTS + AD output missing. MIKE 1D LTS AD not reading Events Loads in the LTS Statistics specifications and AD component results are not written down to erf-file	Fixed
MIKE 1D	Die Verwendung von MIKE 1D LTS mit Colebrook-White Rauheit ergibt einen Fehler nach Abschluss der Berechnung..	Fixed
MIKE 1D	MIKE 1D - LTS behandelt START und STOP Datum/Uhrzeit für die Simulation nicht korrekt. Wenn die Start- und Endzeit der Simulation geändert wird (z.B. nur ein Jahr, z.B. 1974, bei Verwendung derselben kompletten Jobliste 1936-1979), schlägt die Simulation fehl und gibt den folgenden Fehler aus: Unexpected simulation launcher exception.	Fixed
MIKE 1D	Die Aufteilung der MIKE 1D Parallelisierung überspringt einige Schritte gegenüber der "Standard"-Parallelisierung. Structure quantities are not updated with end-of-time step water levels Numerical water is reported incorrectly. Updates to the HDDomain method is required	Fixed
MIKE 1D	Viele Systeme mit aktiviertem Hyper-Threading arbeiten schlecht, weil die Berechnung mit zu vielen Threads läuft. Ein automatischer Ansatz zur Überprüfung, ob Hyper Threading aktiviert ist, wurde implementiert.	Fixed
MIKE URBAN	The “MOUSEtoSWMM” conversion tool now exports the CRS links as CRS sections in the SWMM converted model	Fixed
MIKE URBAN	MIKE URBAN Lizenzmodule sollten "ausgetauscht" werden, so wie mit MZAPPSHELL or WEST Lizenzmodulen	Fixed
MIKE URBAN	MU Netzneuaufbau braucht eine Option for silent mode...	Fixed
MIKE URBAN ECOLAB	Ein Fehler beim Lesen bestimmter Konstanten mit in-builts IDs wurde behoben.	Fixed
Water Distribution	The STATUS section of the original INP file has items that are not correctly processed by MU i.e. the status field of links. As a result of that the above links (valves, pumps) are initially OPEN in MU while they should be CLOSED as in the original file. Attached is the original INP file. The above CLOSED links must appear in the INP file that is exported from MU.	Fixed
Water Distribution	EPANET 2.0012 und MIKE URBAN WD erzeugen unterschiedliche Ergebnisse auf der Grundlage der gleichen Eingabedaten für ein bestimmtes Modell	Fixed
Water Distribution	Water Distribution Ergebnisstatistiken werden nicht aktualisiert, wenn sie mehrfach bei Aktualisierungen/Änderungen ausgeführt werden.	Fixed

MIKE URBAN 2017, Service Pack 1 (SP1), Oktober 2017

Modul/Typ	Neues Feature/Fehler	Status
General	MU 2017 has been upgraded to support ArcGIS 10.5.1	New Feature
MIKE 1D	MU RR Model B Horton infiltration has been reviewed and fixed, especially with regard to evaporation and infiltration. Some of the changes are: the order of draining, limitation of infiltration by rain has been disabled, and recovering of infiltration potential has been updated.	New Feature
Collection System	The SWMM module has been updated to import different types of time patterns	New Feature
Water Distribution	Enhanced the possibility to enter values in the dialog if numbers less than 0.000 for PID Parameters. On top of this the PID computation has been reviewed and updated.	New Feature
MIKE 1D	MIKE 1D LTS ERF file reports the specified event definition properly.	Fixed
MIKE 1D	MIKE 1D saves all results according to the User Specified result file specification including velocity and discharge, weir discharge and pump discharge.	Fixed
MIKE 1D	MIKE 1D LTS crashing problem due to an extremely large result file and use of the memory has been addressed and fixed with this Service Pack.	Fixed
MIKE 1D	OneDayProfile validation for some specific DWF models have been fixed. Upgrading the way MIKE 1D handles Diurnal Pattern Profiles.	Fixed
MIKE 1D	MIKE 1D AD computations have been fixed avoiding that they go through non-return valves.	Fixed
MIKE 1D	A problem with the diagnostics for a pump stop level during startup has been fixed.	Fixed
MIKE 1D	MIKE 1D Storm water inlets calculates derivatives correctly now.	Fixed
MIKE 1D	Model C has been fixed to function properly when the lag time has not been specified	Fixed
MIKE 1D	MIKE 1D Control module has been enabled to cope with a function named “Change” which was not previously recognized	Fixed
Water Distribution	Issues related to pipe roughness calibration	Fixed1) siehe MIKE URBAN hotfix 19-07-2017; diese Zeile fehlt in den originalen Release Notes

MIKE URBAN 2017, April 2017

Modul/Typ	Fehler/Neues Feature	Status
General	Upgrade of MIKE URBAN to support ArcGIS 10.5 MIKE 1D now runs in 64 bit when executed from MIKE URBAN. This leads to better utilisation of your hardware, in particularly, when working with large data sets and models.	New Feature
Building and maintaining models	Enhanced hydrogen sulphide modelling. The H2S ECO Lab template have been enhanced, supporting the simulation of sulphide precipitation by dosing with ferrous and ferric based chemicals ECO Lab template is included for modeling H2S concentration	New Feature
MIKE 1D	A series of improvements on the MIKE1D engine focusing on even better performance and stability	New Feature
MOUSE	Pump Emergency Storage Tool now available (for the MOUSE Engine only).	New Feature
Model Manager	SWMM mode, improved importing capabilities of multiple time patterns and large time series	Fixed
Model Manager	SWMM longitudinal profile plots have been corrected for animated result presentation	Fixed
Model Manager	Catchment processing tool has been improved to handle large setups	Fixed
Collection System	Graphical selection of nodes covering soakaway type to create catchment connections	Fixed
Collection System	CS SWMM values specified in Areal Depletion under Hydrology|Climatology are now exported to the .inp file	Fixed
MIKE 1D engine	Computation of Horton´s infiltration has been improved for runoff model C	Fixed
MIKE 1D engine	MIKE 1D a problem with the engine skipping jobs in LTS simulations have been fixed	Fixed
MIKE 1D MIKE View	Ergebnisse einer LTS-Simulation, die mit MIKE 1D durchgeführt worden ist, können nun in MIKE View dargestellt werden	Fixed
MIKE 1D engine	NAM/RDI and TA/RDI html summary file volume balance has been corrected	Fixed
MIKE 1D engine	Runoff model C2 calculation has been improved to correctly run the simulation in cases when the lag time has not been specified	Fixed
Water Distribution	A problem occurring when the file path is too long has been fixed	Fixed