Neu in MIKE URBAN Version 2017

MIKE URBAN 2017, April 2017

Modul/Typ	Fehler/Neues Feature	Status
General	Upgrade of MIKE URBAN to support ArcGIS 10.5 MIKE 1D now runs in 64 bit when executed from MIKE URBAN. This leads to better utilisation of your hardware, in particularly, when working with large data sets and models.	New Feature
Building and maintaining models	Enhanced hydrogen sulphide modelling. The H2S ECO Lab template have been enhanced, supporting the simulation of sulphide precipitation by dosing with ferrous and ferric based chemicals ECO Lab template is included for modeling H2S concentration	New Feature
MIKE 1D	A series of improvements on the MIKE1D engine focusing on even better performance and stability	New Feature
MOUSE	Pump Emergency Storage Tool now available (for the MOUSE Engine only).	New Feature
Model Manager	SWMM mode, improved importing capabilities of multiple time patterns and large time series	Fixed
Model Manager	SWMM longitudinal profile plots have been corrected for animated result presentation	Fixed
Model Manager	Catchment processing tool has been improved to handle large setups	Fixed
Collection System	Graphical selection of nodes covering soakaway type to create catchment connections	Fixed
Collection System	CS SWMM values specified in Areal Depletion under Hydrology|Climatology are now exported to the .inp file	Fixed
MIKE 1D engine	Computation of Horton´s infiltration has been improved for runoff model C	Fixed
MIKE 1D engine	MIKE 1D a problem with the engine skipping jobs in LTS simulations have been fixed	Fixed
MIKE 1D MIKE View	Ergebnisse einer LTS-Simulation, die mit MIKE 1D durchgeführt worden ist, können nun in MIKE View dargestellt werden	Fixed
MIKE 1D engine	NAM/RDI and TA/RDI html summary file volume balance has been corrected	Fixed
MIKE 1D engine	Runoff model C2 calculation has been improved to correctly run the simulation in cases when the lag time has not been specified	Fixed
Water Distribution	A problem occurring when the file path is too long has been fixed	Fixed