Neu in MIKE URBAN Version 2017

MIKE URBAN 2017, Service Pack 1 (SP1)

Neu in MIKE URBAN SP1:

- Unterstützung der neueren ArcGIS Version 10.5.1

- MIKE 1D Oberflächenabfluss Modell B (Kinematische Welle) wurde überprüft und einer kompletten Überarbeitung unterzogen, insbesondere in Bezug auf Verdunstung, Infiltration und die Horton-Ansätze. Die folgenden Änderungen sind enthalten:

Reihenfolge der Drainage hat sich geändert

Die Begrenzung der Versickerung durch Regen wurde deaktiviert

Die Wiedergewinnung des Versickerungspotentials wurde aktualisiert

Eine weitere Optimierung der LTS-Simulationen mit MIKE 1D wurde durchgeführt, um kleinere Ergebnisdateien zu erzeugen und den Systemspeicher optimal zu nutzen.

Modul/Typ	Neues Feature/Fehler	Status
General	MU 2017 has been upgraded to support ArcGIS 10.5.1	New Feature
MIKE 1D	MU RR Model B Horton infiltration has been reviewed and fixed, especially with regard to evaporation and infiltration. Some of the changes are: the order of draining, limitation of infiltration by rain has been disabled, and recovering of infiltration potential has been updated.	New Feature
Collection System	The SWMM module has been updated to import different types of time patterns	New Feature
Water Distribution	Enhanced the possibility to enter values in the dialog if numbers less than 0.000 for PID Parameters. On top of this the PID computation has been reviewed and updated.	New Feature
MIKE 1D	MIKE 1D LTS ERF file reports the specified event definition properly.	Fixed
MIKE 1D	MIKE 1D saves all results according to the User Specified result file specification including velocity and discharge, weir discharge and pump discharge.	Fixed
MIKE 1D	MIKE 1D LTS crashing problem due to an extremely large result file and use of the memory has been addressed and fixed with this Service Pack.	Fixed
MIKE 1D	OneDayProfile validation for some specific DWF models have been fixed. Upgrading the way MIKE 1D handles Diurnal Pattern Profiles.	Fixed
MIKE 1D	MIKE 1D AD computations have been fixed avoiding that they go through non-return valves.	Fixed
MIKE 1D	A problem with the diagnostics for a pump stop level during startup has been fixed.	Fixed
MIKE 1D	MIKE 1D Storm water inlets calculates derivatives correctly now.	Fixed
MIKE 1D	Model C has been fixed to function properly when the lag time has not been specified	Fixed
MIKE 1D	MIKE 1D Control module has been enabled to cope with a function named “Change” which was not previously recognized	Fixed

MIKE URBAN 2017, April 2017

Modul/Typ	Fehler/Neues Feature	Status
General	Upgrade of MIKE URBAN to support ArcGIS 10.5 MIKE 1D now runs in 64 bit when executed from MIKE URBAN. This leads to better utilisation of your hardware, in particularly, when working with large data sets and models.	New Feature
Building and maintaining models	Enhanced hydrogen sulphide modelling. The H2S ECO Lab template have been enhanced, supporting the simulation of sulphide precipitation by dosing with ferrous and ferric based chemicals ECO Lab template is included for modeling H2S concentration	New Feature
MIKE 1D	A series of improvements on the MIKE1D engine focusing on even better performance and stability	New Feature
MOUSE	Pump Emergency Storage Tool now available (for the MOUSE Engine only).	New Feature
Model Manager	SWMM mode, improved importing capabilities of multiple time patterns and large time series	Fixed
Model Manager	SWMM longitudinal profile plots have been corrected for animated result presentation	Fixed
Model Manager	Catchment processing tool has been improved to handle large setups	Fixed
Collection System	Graphical selection of nodes covering soakaway type to create catchment connections	Fixed
Collection System	CS SWMM values specified in Areal Depletion under Hydrology|Climatology are now exported to the .inp file	Fixed
MIKE 1D engine	Computation of Horton´s infiltration has been improved for runoff model C	Fixed
MIKE 1D engine	MIKE 1D a problem with the engine skipping jobs in LTS simulations have been fixed	Fixed
MIKE 1D MIKE View	Ergebnisse einer LTS-Simulation, die mit MIKE 1D durchgeführt worden ist, können nun in MIKE View dargestellt werden	Fixed
MIKE 1D engine	NAM/RDI and TA/RDI html summary file volume balance has been corrected	Fixed
MIKE 1D engine	Runoff model C2 calculation has been improved to correctly run the simulation in cases when the lag time has not been specified	Fixed
Water Distribution	A problem occurring when the file path is too long has been fixed	Fixed