Neu in Release 2019 Update 1

Modul/Typ	Neues Feature/Fehler	Status
General	MIKE URBAN is updated to ArcGIS 10.7	New Feature
General	MIKE URBAN updated to support SWMM5.1.013	New Feature
MIKE 1D	MIKE 1D gridded rain, dfs2 orientation in degrees used as radians	Fixed
MIKE 1D does not read BRANCH_MIN_H_REL and BRANCH_MIN_H_ABS from dhiapp.ini	Fixed
Volume available for pumping includes discharge from connected structures	Fixed
Runtime stop criterion type "Filling degree" does not work with weirs/orifices/pumps in MIKE 1D	Fixed
MIKE 1D ignores max-min timestep parameter in the joblist file of LTS calculation	Fixed
Model Manager	Simplification Wizard does not visualize new demand allocation connection lines correctly	Fixed
Remove multiple results at one click in MIKE URBAN Longitudinal Profiles	Fixed
Model Manager (EPANET)	Simplification Wizard, demands not moved downstream when there are two or more demands connected to a junction.	Fixed
CS-Pipe Flow	Suffix “CatchmentDischarge” is added to the catchment MUID disabling MIKE1D from reading the information in Boundary Conditions	Fixed
Model Manager (SWMM5)	Example1 cannot complete simulation with latest SWMM5 engine version	Fixed
Crash when trying to browse a file to import in a specific combination in the Import / Export wizard	Fixed
Exception error when trying to import from specific inp file	Fixed
Catchment Slope and Length: Exception error when clicking No in the Warning dialog	Fixed
Model Manager	Can't load specific MIKE 1D rainfall runoff result file	Fixed
Path for Long profile is not fully controllable and wrong path is loaded	Fixed
MU DFS2 support does not work with ArcGIS 10.6.1	Fixed
Model Manager (EPANET)	Demand Statistic dialog does not have copy/paste options	Fixed
Model Manager (MOUSE/MIKE1D)	Curves and Relations Dialog, The third column 'As' is not hidden, appears in all curves that should only have two columns	Fixed
CS-Pipe Flow (MIKE 1D)	MIKE 1D merges the catchment ID and the linked boundary condition type into a single non existing MUID when aiming to run the RDI simulation - causing the simulation to stop	Fixed
Cannot derive some results from MIKE 1D network calculation results *.res1d	Fixed
Model Manager	MU Project Check Tool does not check for duplicate node MUIDs	Fixed
CS-Pipe Flow	Error that MIKE URBAN loads a MIKE 1D result file as soon as a simulation is started, if the previous result file is stored in the same folder as the setup	Fixed
Model Manager (EPANET)	PID Control dialog - attributes missing in the "Tools / Customize / Custom Units", mw_PID	Fixed
Model Manager (MIKE1D)	Problems with MOUSE engine after upgrading a model from MIKE URBAN 2016 to MIKE URBAN 2017	Fixed
Model Manager	Problem with SWQ Editor functionality with linking to specified Q-H relation specified in GUI	Fixed
CS-Pipe Flow	MIKE URBAN - UHM model result incorrect if simulation time shorter than lag time	Fixed
Model Manager (EPANET)	Option for user defined prefix for MUIDs when adding new features	Fixed
Model Manager (SWMM5)	Export of transect X and Z values are swapped	Fixed
CS-Pipe Flow (MIKE 1D, LTS)	MIKE 1D LTS: including AD statistics [Discharge_Load_Out] is ommitted from ERF file	Fixed
CS-Pipe Flow (MIKE 1D, LTS)	MIKE 1D LTS: statistics for AD components not related to event definition	Fixed
CS-Pipe Flow (MIKE1D)	MIKE 1D truncates RTCFunction.TSConnection1	Fixed
mdb template (Primary) should be exported to gdb template.	Fixed
Model Manager	Option for user defined prefix for MUIDS when adding new features.	Fixed
Model Manager (SWMM5)	Problem with loading result items	Fixed
Model Manager (EPANET)	The greyed out field beside diameter displaying "diameter - diameter - wall thickness" should be "diameter = diameter – 2 * wall thickness".	Fixed
Model Manager 1) 2D Flood	Changes to the SimulationID does not change the result filename for the .dfs2 in flood simulation causing overwrite of existing result files	Fixed
Generate Fish Extent causes MIKE URBAN crash, if decimal separator is set to comma and not dot	Fixed
Changing the Node ID does not cascade to changing the Node ID for the coupled cells	Fixed
Model Manager	Update of catchment parameters fails (msm_HModA) in the Import / Export tools	Fixed
Model Manager (2D FLOOD)	"Node Water Level" result list for MIKE 1D flood results viewed in MIKE URBAN incorrectly offers both node and M21 node levels	Fixed
Model Manager	Export to ISYBAU format is not working	Fixed
Model Manager	The volume graph for basin storage should be drawn based on calculating many points covering the range of the specified table	Fixed
Model Manager (CS-Pipe Flow)	MIKE URBAN and ECOLAB - editing built-in constants. The editor field "Global value" (attribute msm_EcolabCoeffvalue) should be disabled if msm_EcolabBuildInID <> -1, which means the values come directly from ECO Lab	Fixed
Model Manager (CS-Pipe Flow)	Improvement of the syntax in the LTS statistics result file ERF	Fixed
Problem with MIKE1D engine writing LTS result file ERF in binary format	Fixed
Model Manager (SWMM5)	SWMM5 should support routing steps in decimals	Fixed
Model Manager (CS-Pollution Transport)	Catchment processing SWQ concentrations: the tool does not work for multiple components	Fixed
Model Manager	After MIKE 1D simulations, result files are not auto loaded	Fixed
Model Manager (2D FLOOD)	Error in 2D OverlandFlow Example with reading Band_1 in DEM.dfs2	Fixed
Model Manager (CS-Pipe Flow)	Error in MIKE1D engine requiring a Q-H relation table having at least three entries specified – two entries is enough	Fixed

Neu in MIKE URBAN Version 2019

Modul/Typ	Neues Feature/Fehler	Status
Import/Export	Export to ISYBAU format is not working	New Feature
Model Manager	mdb template (Primary) should be exported to gdb template.	Fixed
MU DFS2 support does not work with ArcGIS 10.6.1	Fixed
Option for user defined prefix for MUIDS when adding new features.	New Feature
Path for Long profile is not fully controllable and wrong path is loaded	Fixed
Remove multiple results at one click in MIKE URBAN Longitudinal Profiles	Fixed
Model Manager Tools	Simplification Wizard, demands not moved downstream when there are two or more demands connected to a junction.	Fixed
Simplification Wizard does not visualize new demand allocation connection lines correctly	Fixed
MU Project Check Tool does not check for duplicate node MUIDs	Fixed
Collection System	Curves and Relations Dialog, The third column 'As' is not hidden, appears in all curves that should only have two columns	Fixed
MIKE URBAN - UHM model result incorrect if simulation time shorter than lag time	Fixed
Problems with MOUSE engine after upgrading a model from MIKE URBAN 2016 to MIKE URBAN 2017	Fixed
The volume graph for basin storage should be drawn based on calculating many points covering the range of the specified table	Fixed
Update of catchment parameters fails (msm_HModA) in the Import / Export tools	Fixed
Problem with SWQ Editor functionality with linking to specified Q-H relation specified in GUI	Fixed
Catchment processing SWQ concentrations: the tool does not work for multiple components	Fixed
MIKE URBAN and ECOLAB - editing built-in constants. The editor field "Global value" (attribute msm_EcolabCoeffvalue) should be disabled if msm_EcolabBuildInID <> -1, which means the values come directly from ECO Lab	Fixed
MIKE 1D	Suffix “CatchmentDischarge” is added to the catchment MUID disabling MIKE1D from reading the information in Boundary Conditions	Fixed
After MIKE 1D simulations, result files are not auto loaded	Fixed
Can't load specific MIKE 1D rainfall runoff result file	Fixed
MIKE 1D merges the catchment ID and the linked boundary condition type into a single non existing MUID when aiming to run the RDI simulation - causing the simulation to stop	Fixed
Cannot derive some results from MIKE 1D network calculation results *.res1d	Fixed
Error in MIKE1D engine requiring a Q-H relation table having at least three entries specified -- two entries is enough	Fixed
Error that MIKE URBAN loads a MIKE 1D result file as soon as a simulation is started, if the previous result file is stored in the same folder as the setup	Fixed
MIKE 1D truncates RTCFunction.TSConnection1	Fixed
LTS	Improvement of the syntax in the LTS statistics result file ERF	Fixed
MIKE 1D LTS	Including AD statistics [Discharge_Load_Out] is ommitted from ERF file	Fixed
Problem with MIKE1D engine writing LTS result file ERF in binary format	Fixed
Statistics for AD components not related to event definition	Fixed
Water Distribution	PID Control dialog - attributes missing in the "Tools | Customize | Custom Units", mw_PID	Fixed
The greyed out field beside diameter displaying "diameter - diameter - wall thickness" should be "diameter = diameter -- 2 * wall thickness".	Fixed
EPANET	Demand Statistic dialog does not have copy/paste options	Fixed
Option for user defined prefix for MUIDs when adding new features	Fixed
SWMM5	SWMM5 should support routing steps in decimals	Fixed
Catchment Slope and Length: Exception error when clicking No in the Warning dialog	Fixed
Crash when trying to browse a file to import in a specific combination in the Import / Export wizard	Fixed
Example1 cannot complete simulation with latest SWMM5 engine version	Fixed
Exception error when trying to import from specific inp file	Fixed
Export of transect X and Z values are swapped	Fixed
Problem with loading result items	Fixed
2D FLOOD	"Node Water Level" result list for MIKE 1D flood results viewed in MIKE URBAN incorrectly offers both node and M21 node levels	Fixed
Changes to the SimulationID does not change the result filename for the .dfs2 in flood simulation causing overwrite of existing result files	Fixed
Changing the Node ID does not cascade to changing the Node ID for the coupled cells	Fixed
Error in 2D OverlandFlow Example with reading Band_1 in DEM.dfs2	Fixed
Generate Fish Extent causes MIKE URBAN crash, if decimal separator is set to comma and not dot	Fixed