Neu in MIKE+ 2022

⯇ Zurück zu MIKE+

Unsere Vision ist, den Wasserkreislauf ganzheitlich abzubilden. Neben urbanen Funktionen, wie dem Abwassernetz und der Wasserversorgung, bietet MIKE+ auch die Möglichkeiten für die GIS-basierte Simulation von Langzeitserien, Echtzeitsteuerung, Oberflächenabfluss sowie Stoff- und Sedimenttransport. Zusätzlich bieten wir die Möglichkeit der Löschfallsimulation.

Mit jedem neuen Release gibt es in der Siedlungswasserwirtschaft und der Benutzeroberfläche zahlreiche Neuerungen. Folgende Seite listet die wichtigsten Verbesserungen und Neuheiten von MIKE+ 2022 (ohne Anspruch auf Vollständigkeit).

On demand Webinar MIKE+ 2022

Angaben zu älteren Versionen finden Sie in der MIKE+ Versionsgeschichte.

Neu: Export von Karten- und Ergebnisdaten nach CAD

Ein Export von Karten- und Ergebnisdaten aus MIKE+ in die Formate .dwg und .dfx ist nun möglich. Sie können Kartendaten oder Längenschnitte per Mausklick exportieren.

Neu: Messwerkzeug

Mit dem Update auf MIKE+ 2022 wurde auf populären Kundenwunsch hin ein Messwerkzeug eingeführt.

Neu: Ergebnistabelle und Statistiken

In der Siedlungsentwässerung haben Sie die Möglichkeit, statistische Kennzahlen, wie Minima, Maxima oder Durchschnitte, sowie akkumulierte Werte zu berechnen. Sie können diese für Einzugsgebiete und Netzwerkresultate berechnen.

Zur besseren Ergebnisübersicht haben Sie mit dem release von MIKE+ 2022 die Möglichkeit, eine Tabelle zu erstellen. Es vereint Daten aus Ihren Modelldaten und den (statistischen) Resultaten. Diese Tabelle können Sie kopieren und sofort in Excel oder anderen Kalkulationsprogrammen verwenden.

Neu: Import - Zusammenfügen mehrerer Datenbanken

Beim Import von Daten in Ihr MIKE+ Projekt können Sie durch die Neuerungen im Automap-Tool mehrere Datenbanken automatisch zusammenführen.

Mit Hilfe des Import-/ Exporttools können Sie Datenbanken ab MIKE+ 2022 über die Asset-ID Daten aus verschiedenen Datenbanken Updaten. Zuvor war das nur über die MUID möglich.

Das Import-/ Exporttool ermöglicht es Ihnen mit dem Update, Punkte aus CAD-Blöcken zu importieren.

Neu: Modell- und Ergebnisbericht

Durch den Modell- und Ergebnisbericht haben Sie die Möglichkeit, aus den Daten der *.squlite, wie Asset-ID oder Beschreibung, und der *.res1d und anhängenden statistischen Berechnungen, eine Tabelle zu erstellen.

Neu: Vereinfachung Fließpfadanalyse

Sowohl in der Wasserversorgung, als auch in der Siedlungsentwässerung wurde die Fließpfadanalyse vereinfacht. Sie haben nun leichter die Möglichkeit, für Sie irrelevante Informationen bei der Analyse auszublenden.

Die Verbesserungen in der Ergebnisdarstellung führen dazu, dass Sie eine bessere Übersicht über Ihre Resultate erlangen, noch bevor Sie einen Output generieren. Zusätzlich wurden einige Bugs ausgemärzt.

Wasserversorgung

Online Analyse: MIKE+ Daten können zu einem SCADA Kontrollsystem hinzugefügt werden. Das Werkzeug ist für die Analysemöglichkeiten unseres verbesserten Waternet Advisors ausgelegt. Die Daten werden über ein Online-Analyse Tool eingefügt.

Pumpen- und Ventiloptimierung: Das neue Analysetool zur Pumpen- und Ventiloptimierung erlaubt Ihnen, den idealen Betriebszustand zu ermitteln. Durch diese Neuerung können in weiterer Folge Einsparungs- oder Energieoptimierungspotentiale ermittelt werden.

Eine weitere Neuerung in MIKE+ 2022 gibt Ihnen die Möglichkeit, den Energieverbrauch, Kostenanalysen oder die CO2 Äquivalente der Betriebszustände zu analysieren.

Siedlungsentwässerung

Vergleichen von Ergebnissen

Sie haben ein Stand-Alone Werkzeug zur Verfügung, das es Ihnen ermöglicht, Varianten eines Modells direkt mit einander zu vergleichen. Über die Befehlszeile finden Sie das Tool Result Verification:

Sie können das Werkzeug für Variantenstudien einsetzen oder alte Modelle mit Ihren Berechnungen in MIKE+ 2022 vergleichen. Eine weitere Einsatzmöglichkeit bietet sich mit dem Vergleich von verschiedenen Netzdaten nach einem Update an. Das Werkzeug informiert Sie automatisch über grobe Differenzen zwischen Ihren Varianten.

Eine Visualisierung und ein Vergleich der Ergebnisse von alten Modellen und neuen Modellen ist durch ein neues Asset Management System ​möglich.

2D Überflutungen

Kopplung von Advektions-Dispersions Berechnung 1D mit 2D

MIKE ZERO Launch: Simulationen sind nun über MIKE ZERO Launch möglich und erlauben Ihnen so, neben einer laufenden Simulation den Model Manager frei zu halten. Somit können Sie den Model Manager trotz laufender Simulation auf einem anderen Endgerät verwenden.

Fließgewässer Import: Sie können nun Daten aus MIKE HYDRO River, MIKE 11 und Oracle Spatial importieren.

MIKE+ 2022 Release Notes

Modul/Typ	Fehler/Neues Feature	Status
General	SWMM model networks can now be coupeld to a 2D overland model. In this version, couplings to the 2D model are only available with nodes, and coupling of water quality components is not supported	New Feature
General	Map data from MIKE+ can now be exported to CAD files (.dwg and .dxf formats), using the import and export tool.	New Feature
General	Longitudiunal profile plots can be now exported to CAD files (.dwg format).	New Feature
General	From the "Import and Export" tool, it is now possible to import data from an Oracle spatial database-	New Feature
General	Connecting to a WMS server to display background layers now allow connecting through a proxy server	New Feature
General	A new "Measure" tool is avialable in the ribbon bar, in the Map tab. It allows measuring distances on the map along segments or plylines, as well as polygons' areas.	New Feature
General	The "Export map" button has been added to the ribbon, in the Map-tab. It can be used to save the map layout to an image file.	New Feature
General	The "Import and Export" tool can be executed from a command line, reading the import/export configuration from a configuration file.	New Feature
General	A new "Automap" button has been added to the "Import and Export" tool. When importing data from MIKE+ projects to an other MIKE+ project, this button will create all sections corresponding to all relevant tables in the MIKE+ database for the active working mode and will populate them with the proper assignments. Duplicates will be renamed.	New Feature
General	In the "Import and Export" tool, a new job property called "Source text format" has been added. This option applies when converting input strings (texts) to numbers, and controls how the decimal seperator is identified.	New Feature
General	A new function called DoubleFromString has been added to the Expression editor, to convert input string (text) data to numerical values and controlling the format of the decimal seperator in the input text. It can be e.g. be used in the "Field calculator" or the "Import and Export" tool.	New Feature
General	The date and time of results shown in the "Property and result explorer is now synchronised with the date and time of results shown on the map.	New Feature
General	It is now possible to export simulation files and run simulations from a command line also for Water Distribution and SWMM model types.	New Feature
General	The tool "Clone and repair database", available in the File menue, may be used with damaged and corrupt databases. It will create a new database but without the damaged tables, which can be then populated again manually.	New Feature
General	A default unit system can now be selected from the "User preferences dialog, to choose between SI and US unit systems. It will especially control in which unit system the results are shown, when no model database is opened.	New Feature
General	In the "Model and result report" tool "Joins" can now merge data from model tables and results in a common table of the report. A new "Time step" option also allows adding a column to the join table, with results from a selected time step.	New Feature
General	In "Rivers, collection systems and overland flows" mode, closing MIKE+ while a simulation is running will offer an option to continue the simulation outside of the MIKE+ application. This option can be used to release the license module of the user interface while running a simulation.	New Feature
Collection System and Rivers	A new "Statistics" content type can be selected for catchments and network result files. This type of result file stores max / min / average values and time of max/ min value, as well as accumulated values for the relevant result items, computed throughout the simulation. These statistics are computed during the simulation and therefore do not depend on a storing frequency of the results.	New Feature
Collection System	A new "Results differences" tool is available in the "Results" tab in the ribbon. This tool is designed for comparing results from different variants of hydraulic network simulations, and report any significant difference of result. This may e. g. be used when comparing results from a former version of a model and results from a new version updated with the latest information from an asset management system. The tool allows you to quickly identify locations where results differences are observed, and visualise and vompare results at these locations. It is not necessary to have a model database opened for using the tool.	New Feature
Collection System	An "initial level" can now be specified in the weir's and orifices' properties, to control the elevation of structures controlled by control rules at the start of the simulation.	New Feature
Rivers	Several new types of structures are now available for river networks: Pumps, Bridge structures, Dambrakes, Tabulated structures, and user-defined Energy losses.	New Feature
Rivers	River models previously created with MIKE HYDRO River or MIKE 11 can now be imported automatically into MIKE+, from the File\ Import menu. Please note that the import is limited to the river functionalities currently supported in MIKE+ (mainly the river and catchments definitions as well as structures and boundary conditions), whereas some functionalities remain unsupported for now in MIKE+ and are ignored during the import (e. g. storages, multiple zone resistance and time-varying resistance factors, variables, side structures, etc.). Before importing a river model, make sure that all expected river functionalities are available in MIKE+ and check for possible warnings in the Log after the import.	New Feature
2D overland	Improved performance for 2D overland applications using GPU acceleration: Tuning of timings and numerous small tweaks, OpenMP parallelization for pre-processing of infrastructure, Pre-processing of boundary conditions (initialization), Optimised data transfer on 2D flood statistics results; In addition a new dynamic list approach is used together with optimised gradient calculation for forcing calculations.	Improvement
2D overland	Coupling of Advection- Dispersion components is now possible also when coupling the 1D network to a MIKE 21 FM or MIKE 3 FM file.	New Feature
SWMM	The "Topology Repair" tool is now also available for SWMM model networks.	New Feature
Water Distribution	A new "optimisation" special analysis has been added. It is used to optimise pumps and valves' behavior to meet e. g. target water depth, pressure or flow in the network.	New Feature
Water Distribution	A new "Online analysis" special analysis has been added. It is used to map the model data from MIKE+ to SCADA system's data, especially for use in Water Distribution Online.	New Feature